# Constant Field Values

## Contents

- voltage.controllers.*
- voltage.core.*
- voltage.processors.*

## voltage.controllers.*

- voltage.controllers.ADSREnvelope
  Modifier and Type
  Constant Field
  Value
  `public final double`
  `MIN_TIME`
  `0.0`

## voltage.core.*

- voltage.core.Values
  Modifier and Type
  Constant Field
  Value
  `public static final double`
  `HALF_PI`
  `1.5707963267948966`
  `public static final double`
  `MsPerSample`
  `0.020833333333333332`
  `public static final double`
  `PI`
  `3.141592653589793`
  `public static final double`
  `SampleRate`
  `48000.0`
  `public static final double`
  `SamplesPerMs`
  `48.0`
- voltage.core.VoltageModule
  Modifier and Type
  Constant Field
  Value
  `public static final long`
  `GUI_UPDATE_TIME`
  `50L`
- voltage.core.VoltageObjects
  Modifier and Type
  Constant Field
  Value
  `public static final int`
  `MAX_NUM_BUSES`
  `32`
  `public static final int`
  `MAX_NUM_POLY_VOICES`
  `16`
  `public static final int`
  `NumberOfInputs`
  `4`
  `public static final int`
  `NumberOfOutputs`
  `8`

## voltage.processors.*

- voltage.processors.BiQuadFilter
  Modifier and Type
  Constant Field
  Value
  `public static final double`
  `M_LN2`
  `0.6931471805599453`